
Lab - Implement EIGRP for IPv6 (Instructor Version)

**Instructor Note**: Red font color or gray highlights indicate text that appears in the instructor copy only.

# Topology



# Addressing Table

| Device | Interface | IPv6 Address/Prefix Length | Link Local Address |
| --- | --- | --- | --- |
| R1 | E0/0 | 2001:db8:cafe:1::1/64 | fe80::1:1 |
| R1 | E0/1.1 | 2001:db8:acad:1::1/64 | fe80::1:2 |
| R1 | E0/1.2 | 2001:db8:acad:2::1/64 | fe80::1:3 |
| R2 | E0/0 | 2001:db8:cafe:1::2/64 | fe80::2:1 |
| R2 | E0/1 | 2001:db8:cafe:2::2/64 | fe80::2:2 |
| R2 | Loopback 0 | 2001:db8:ff:999:153/64 | fe80::2:3 |
| R2 | Loopback 1 | 2001:db8:cede::1/64 | fe80::2:4 |
| R2 | Loopback 2 | 2001:db8:cede:1::1/64 | fe80::2:5 |
| R3 | E0/0 | 2001:db8:cafe:2::1/64 | fe80::3:1 |
| R3 | E0/1 | 2001:db8:acad:3::1/64 | fe80::3:2 |
| R3 | Loopback 1 | 2001:db8:abcd:8::1/64 | fe80::3:3 |
| R3 | Loopback 2 | 2001:db8:abcd:9::1/64 | fe80::3:4 |
| R3 | Loopback 3 | 2001:db8:abcd:10::1/64 | fe80::3:5 |
| R3 | Loopback 4 | 2001:db8:abcd:11::1/64 | fe80::3:6 |
| R3 | Loopback 5 | 2001:db8:abcd:12::1/64 | fe80::3:7 |
| D2 | E1/1 | 2001:db8:acad:1::2/64 | fe80::d2:1 |
| D2 | E1/0 | 2001:db8:acad:3::2/64 | fe80::d2:2 |
| PC1 | NIC | SLAAC | EUI-64 |

# Objectives

**Part 1: Build the Network and Configure Basic Device Settings**

**Part 2: Implement EIGRP for IPv6 and Named EIGRP**

**Part 3: Tune and Optimize EIGRP for IPv6**

# Background / Scenario

EIGRP for IPv6 has the same overall operation and features as EIGRP for IPv4. However, there are a few major differences between them:

* IPv6 unicast routing must be enabled before the routing process can be configured.
* In the absence of the router having any IPv4 addresses, a 32-bit router ID must be configured for the routing process to start.
* EIGRP for IPv6 is configured directly on the router interfaces.

In this lab, you will configure the network with EIGRP for IPv6. You will also configure passive interfaces, propagate a default route, configure a summary route, implement routing protocol authentication, modify load balancing, and filter routes with a prefix list.

**Note**: This lab is an exercise in configuring the options available with EIGRP for IPv6. It does not necessarily reflect implementation best practices.

**Note**: The routers used with CCNP hands-on labs are Cisco 4221 with Cisco IOS XE Release 16.9.4 (universalk9 image). The switches used in the labs are Cisco Catalyst 3650 with Cisco IOS XE Release 16.9.4 (universalk9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of the lab for the correct interface identifiers.

**Note**: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.

**Instructor Note**: Refer to the Instructor Lab Manual for the procedures to initialize and reload devices.

# Required Resources

* 3 Routers (Cisco 4221 with Cisco IOS XE Release 16.9.4 universal image or comparable)
* 2 Switches (Cisco 3650 with Cisco IOS XE Release 16.9.4 universal image or comparable)
* 1 PC (Choice of operating system with terminal emulation program installed)
* Console cables to configure the Cisco IOS devices via the console ports
* Ethernet cables as shown in the topology

# Instructions

## Build the Network and Configure Basic Device Settings

In Part 1, you will set up the network topology and configure basic settings and interface addressing on routers.

### Cable the network as shown in the topology.

Attach the devices as shown in the topology diagram, and cable as necessary.

### Configure basic settings for each device.

* + - 1. Console into each device, enter global configuration mode, and apply the basic settings. The startup configurations for each device are provided below.

Open configuration window

Router R1

hostname R1

no ip domain lookup

ipv6 unicast-routing

banner motd # R1, Implement EIGRP for IPv6 #

line con 0

exec-timeout 0 0

logging synchronous

exit

line vty 0 4

privilege level 15

exec-timeout 0 0

password cisco123

login

exit

interface E0/0

ipv6 address 2001:db8:cafe:1::1/64

ipv6 address fe80::1:1 link-local

no shutdown

exit

interface E0/1

no ip address

no shutdown

exit

interface E0/1.1

description VLAN 1 Interface

encapsulation dot1q 1

ipv6 address fe80::1:2 link-local

ipv6 address 2001:db8:acad:1::1/64

no shutdown

exit

interface E0/1.2

description VLAN 2 Interface

encapsulation dot1q 2

ipv6 address fe80::1:3 link-local

ipv6 address 2001:db8:acad:2::1/64

no shutdown

exit

end

Router R2

hostname R2

no ip domain lookup

ipv6 unicast-routing

banner motd # R2, Implement EIGRP for IPv6 #

line con 0

exec-timeout 0 0

logging synchronous

exit

line vty 0 4

privilege level 15

exec-timeout 0 0

password cisco123

login

exit

interface E0/0

ipv6 address fe80::2:1 link-local

ipv6 address 2001:db8:cafe:1::2/64

no shutdown

exit

interface E0/1

ipv6 address fe80::2:2 link-local

ipv6 address 2001:db8:cafe:2::2/64

no shutdown

exit

interface loopback 0

description Internet host

ipv6 address fe80::2:3 link-local

ipv6 address 2001:db8:ff:999::153/64

no shutdown

exit

interface loopback 1

ipv6 address fe80::2:4 link-local

ipv6 address 2001:db8:cede::1/64

no shutdown

exit

interface loopback 2

ipv6 address fe80::2:5 link-local

ipv6 address 2001:db8:cede:1::1/64

no shutdown

exit

end

Router R3

hostname R3

no ip domain lookup

ipv6 unicast-routing

banner motd # R3, Implement EIGRP for IPv6 #

line con 0

exec-timeout 0 0

logging synchronous

exit

line vty 0 4

privilege level 15

exec-timeout 0 0

password cisco123

login

exit

interface E0/0

ipv6 address fe80::3:1 link-local

ipv6 address 2001:db8:cafe:2::1/64

no shutdown

exit

interface E0/1

ipv6 address fe80::3:2 link-local

ipv6 address 2001:db8:acad:1::3/64

no shutdown

exit

interface loopback 1

ipv6 address fe80::3:3 link-local

ipv6 address 2001:db8:abcd:8::1/64

no shutdown

interface loopback 2

ipv6 address fe80::3:4 link-local

ipv6 address 2001:db8:abcd:9::1/64

no shutdown

interface loopback 3

ipv6 address fe80::3:5 link-local

ipv6 address 2001:db8:abcd:10::1/64

no shutdown

interface loopback 4

ipv6 address fe80::3:6 link-local

ipv6 address 2001:db8:abcd:11::1/64

no shutdown

interface loopback 5

ipv6 address fe80::3:7 link-local

ipv6 address 2001:db8:abcd:12::1/64

no shutdown

end

Router D1

hostname D1

no ip domain lookup

banner motd # D1, Implement EIGRP for IPv6 #

line con 0

exec-timeout 0 0

logging synchronous

line vty 0 4

privilege level 15

exec-timeout 0 0

password cisco123

login

vlan 2

name HOST-VLAN

interface range E0/0-3, E1/0-3, E2/0-3, E3/0-3

shutdown

exit

interface range E1/1, E1/0

switchport trunk encapsulation dot1q

switchport mode trunk

no shutdown

exit

interface E3/0

switchport mode access

switchport access vlan 2

spanning-tree portfast

no shutdown

exit

end

Router D2

hostname D2

no ip domain lookup

ipv6 unicast-routing

banner motd # D2, Implement EIGRP for IPv6 #

line con 0

exec-timeout 0 0

logging synchronous

exit

line vty 0 4

privilege level 15

exec-timeout 0 0

password cisco123

login

exit

interface range E0/0-3, E1/0-3, E2/0-3, E3/0-3

shutdown

exit

interface E1/1

no switchport

ipv6 address fe80::d1:1 link-local

ipv6 address 2001:Db8:acad:1::2/64

no shutdown

exit

interface E1/0

no switchport

ipv6 address fe80::d1:2 link-local

ipv6 address 2001:db8:acad:3::2/64

no shutdown

exit

end

* + - 1. Set the clock on each device to UTC time.
      2. Save the running configuration to startup-config.

Close configuration window

* + - 1. Verify that PC1 generates an IPv6 address.
      2. Verify that PC1 can ping its default gateway at **fe80::1:3**.

## Implement EIGRP for IPv6 and Named EIGRP

In this part of the lab, you will configure and verify EIGRP in the network. Routers R1 and R3 will used Named EIGRP, while router R2 will use Classic EIGRP. After you have established the network, you will examine the differences in how each version of EIGRP deals with metrics.

For the lab, you will use the Autonomous System number 43 on all routers.

### Configure EIGRP for IPv6 on R2

* + - 1. Start the configuration of Classic EIGRP by issuing the **ipv6 router eigrp 43** command.

Open configuration window

R2(config)# **ipv6 router eigrp 43**

* + - 1. Configure the EIGRP Router ID using the **eigrp router-id** command. Use the number 2.2.2.2 for R2.

R2(config-router)# **eigrp router-id 2.2.2.2**

* + - 1. Identify the interfaces that should be configured with EIGRP and the networks that should be included in the EIGRP topology table. This is done on the interfaces with the **ipv6 eigrp** command.

R2(config)# **interface E0/0**

R2(config-if)# **ipv6 eigrp 43**

R2(config-if)# **exit**

R2(config)# **interface E0/1**

R2(config-if)# **ipv6 eigrp 43**

R2(config-if)# **exit**

R2(config)# **interface loopback0**

R2(config-if)# **ipv6 eigrp 43**

R2(config-if)# **exit**

R2(config)# **interface loopback1**

R2(config-if)# **ipv6 eigrp 43**

R2(config-if)# **exit**

R2(config)# **interface loopback 2**

R2(config-if)# **ipv6 eigrp 43**

R2(config-if)# **end**

* + - 1. Verify the interfaces now involved in EIGRP with the **show ipv6 eigrp interfaces** command.

R2# **show ipv6 eigrp interfaces**

EIGRP-IPv6 Interfaces for AS(43)

Xmit Queue PeerQ Mean Pacing Time Multicast Pending

Interface Peers Un/Reliable Un/Reliable SRTT Un/Reliable Flow Timer Routes

E0/0 0 0/0 0/0 0 0/0 0 0

E0/1 0 0/0 0/0 0 0/0 0 0

Lo0 0 0/0 0/0 0 0/0 0 0

Lo1 0 0/0 0/0 0 0/0 0 0

Lo2 0 0/0 0/0 0 0/0 0 0

Close configuration window

### Configure Named EIGRP for IPv6 on R1 and R3

* + - 1. Start the configuration of Named EIGRP by issuing the **router eigrp [ name ]** command. The name parameter can be a number, but the number does not identify an Autonomous System as it does with Classic EIGRP, it simply identifies the process. For our purposes, name the process **EIGRP\_IPV6**.

Open configuration window

R1(config)# **router eigrp EIGRP\_IPV6**

R1(config-router)#

* + - 1. Enter into address-family configuration mode with the **address-family ipv6 unicast autonomous-system 43** command**.** It is not necessary to configure EIGRP for IPv6 on the interfaces. In named-mode configuration, EIGRP for IPv6 is automatically enabled on all interfaces that are configured with an IPv6 address.

R1(config-router)# **address-family ipv6 unicast autonomous-system 43**

* + - 1. Configure the EIGRP Router ID using the **eigrp router-id** command. Use the number **1.1.1.1**.

R1(config-router-af)# **eigrp router-id 1.1.1.1**

* + - 1. Repeat the configuration process on R3 and D2. For the R3 router ID use **3.3.3.3,** and for the D2 router ID use 132.132.132.132.

### Verify EIGRP for IPv6

* + - 1. A few seconds after configuring the network statements on R1, R3 and D2, you should have seen EIGRP adjacencies being formed, as noted at the console by messages similar to the one below.

\*Mar 9 13:42:47.969: %DUAL-5-NBRCHANGE: EIGRP-IPv6 43: Neighbor FE80::3:2 (Ethernet1/0) is up: new adjacency

* + - 1. To verify that routing is working, ping from PC1 to Interface Loopback 1 on R3 (2001:db8:abcd:8::1). The ping should be successful.
      2. On R1, examine the EIGRP entries in the IPv6 routing table using the **show ipv6 route eigrp** command. As you can see, R1 is aware of all of the networks that have been configured in the topology. The remote networks that were learned from EIGRP and that appear in the routing table were learned from routers R2 and R3 as indicated by the link local address that is displayed for these entries. Note that in some cases, EIGRP for IPv6 has two equal cost routes for a network.

R1# **show ipv6 route eigrp**

IPv6 Routing Table - default - 17 entries

<output omitted>

D 2001:DB8:FF:999::/64 [90/2570240]

via FE80::2:1, Ethernet0/0

D 2001:DB8:ABCD:8::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:9::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:10::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:11::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:12::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ACAD:3::/64 [90/15360]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:CAFE:2::/64 [90/15360]

via FE80::2:1, Ethernet0/0

D 2001:DB8:CEDE::/64 [90/2570240]

via FE80::2:1, Ethernet0/0

D 2001:DB8:CEDE:1::/64 [90/2570240]

via FE80::2:1, Ethernet0/0

* + - 1. Now examine the EIGRP topology table using the **show ipv6 eigrp topology all-links** command. The all-links parameter instructs the router to display routes that are not successors or feasible successors. We will focus on the routes to 2001:db8:abcd:10::/64 and 2001:db8:cafe:2::/64. There are several things to notice.

Remember that the topology table is EIGRP’s database of route information. EIGRP selects the best paths, based on the DUAL algorithm, and offers them to the IP routing table. However, the IP routing table does not have to use those offered paths, because the router may have learned about the same network from a more reliable routing source, which would be a routing source with a lower administrative distance.

R1# **show ipv6 eigrp topology all-links**

EIGRP-IPv6 VR(EIGRP\_IPV6) Topology Table for AS(43)/ID(1.1.1.1)

Codes: P - Passive, A - Active, U - Update, Q - Query, R - Reply,

r - reply Status, s - sia Status

P 2001:DB8:CEDE:1::/64, 1 successors, FD is 328990720, serno 7

via FE80::2:1 (328990720/327761920), Ethernet0/0

P 2001:DB8:CEDE::/64, 1 successors, FD is 328990720, serno 6

via FE80::2:1 (328990720/327761920), Ethernet0/0

P 2001:DB8:ABCD:10::/64, 2 successors, FD is 2048000, serno 16

via FE80::2:1 (2048000/1392640), Ethernet0/0

via FE80::D1:1 (2048000/1392640), Ethernet0/1.1

P 2001:DB8:ACAD:1::/64, 1 successors, FD is 1310720, serno 2

via Connected, Ethernet0/1.1

via FE80::D1:1 (1966080/1310720), Ethernet0/1.1

P 2001:DB8:ABCD:12::/64, 2 successors, FD is 2048000, serno 18

via FE80::2:1 (2048000/1392640), Ethernet0/0

via FE80::D1:1 (2048000/1392640), Ethernet0/1.1

P 2001:DB8:CAFE:2::/64, 1 successors, FD is 1966080, serno 4

via FE80::2:1 (1966080/1310720), Ethernet0/0

via FE80::D1:1 (2621440/1966080), Ethernet0/1.1

P 2001:DB8:ABCD:9::/64, 2 successors, FD is 2048000, serno 15

via FE80::2:1 (2048000/1392640), Ethernet0/0

via FE80::D1:1 (2048000/1392640), Ethernet0/1.1

P 2001:DB8:ABCD:11::/64, 2 successors, FD is 2048000, serno 17

via FE80::2:1 (2048000/1392640), Ethernet0/0

via FE80::D1:1 (2048000/1392640), Ethernet0/1.1

P 2001:DB8:ACAD:2::/64, 1 successors, FD is 1310720, serno 3

via Connected, Ethernet0/1.2

P 2001:DB8:ABCD:8::/64, 2 successors, FD is 2048000, serno 14

via FE80::2:1 (2048000/1392640), Ethernet0/0

via FE80::D1:1 (2048000/1392640), Ethernet0/1.1

P 2001:DB8:CAFE:1::/64, 1 successors, FD is 1310720, serno 1

via Connected, Ethernet0/0

via FE80::2:1 (1966080/1310720), Ethernet0/0

P 2001:DB8:FF:999::/64, 1 successors, FD is 328990720, serno 5

via FE80::2:1 (328990720/327761920), Ethernet0/0

P 2001:DB8:ACAD:3::/64, 1 successors, FD is 1966080, serno 13

via FE80::D1:1 (1966080/1310720), Ethernet0/1.1

We will focus on the routes, highlighted in the above output, to 2001:db8:abcd:10::/64 and 2001:db8:cafe:2::/64. There are several things to notice:

* The entry for the 2001:db8:abcd:10::/64 network shows two successors, while the entry for 2001:db8:cafe:2::/64 shows only one successor. Both entries show two paths. The path with the lowest Feasible Distance (FD) is selected as the successor and is offered to the routing table. For 2001:db8:abcd:10::/64, there are two paths with equal FD, so they are both successors and both are offered to the global routing table. In the case of 2001:db8:cafe:2::/64, the FD is listed as 19660800. The path via fe80::2:1 shows that number as the FD (first number in parentheses). The path via fe80::d1:1 shows an FD of 2621440, which is higher than the current FD. So that path, although valid, is a higher cost path and is not offered to the routing table.
* The FD listed in the topology table does not match the metric listed in the routing table. For 2001:db8:abcd:10::/64, the routing table shows the metric value 16000 while the topology table shows the FD as 2048000. This is due to the routing table having a limit of 4 bytes (32 bits) for metric information, while EIGRP on R1 is using EIGRP wide metrics, which are 64 bits. Wide metrics are used by Named EIGRP by default. To work around the 32-bit metric size limitation in the routing table, EIGRP divides the wide-metric value by the EIGRP\_RIB\_SCALE value, which defaults to 128. The value 2048000 divided by 128 is 16000.

**Note**: A network with mixed EIGRP implementations (Named and Classic in the same routing domain), will have some loss of route clarity, which could lead to sub-optimal path selection. The recommended implementation is to use Named EIGRP in all cases.

* There are no feasible successors listed in the topology table for 2001:db8:abcd:10::/64 or 2001:db8:cafe:2::/64. The feasibility condition requires that the reported distance (RD) to a destination network be less than the current FD for a next-hop to be considered a feasible successor to the route. In the case of 2001:db8:cafe:2::/64, the RD of the path via fe80::d1:1 is listed as 1966080, which is equal to the current FD, which disqualifies this path as a feasible successor. If the path via fe80::2:1 were to be lost, R1 would have to send queries to find a new way to get to 2001:db8:cafe:2::/64. Feasible successors appear only in the topology table. Only successors appear in the routing table.
  + - 1. To see the RIB Scale and metric version values, as well as other protocol information, issue the **show ipv6 protocols | section EIGRP\_IPv6** command.

R1# **show ipv6 protocols | section EIGRP\_IPV6**

EIGRP-IPv6 VR(EIGRP\_IPV6) Address-Family Protocol for AS(43)

Metric weight K1=1, K2=0, K3=1, K4=0, K5=0 K6=0

Metric rib-scale 128

Metric version 64bit

Soft SIA disabled

NSF-aware route hold timer is 240

EIGRP NSF disabled

NSF signal timer is 20s

NSF converge timer is 120s

Router-ID: 1.1.1.1

Topology : 0 (base)

Active Timer: 3 min

Distance: internal 90 external 170

Maximum path: 16

Maximum hopcount 100

Maximum metric variance 1

Total Prefix Count: 13

Total Redist Count: 0

* + - 1. To examine details about a particular path, issue the **show ipv6 eigrp topology [address]** command. Among other things in this output, you can see the values used in calculating the metric.

R1# **show ipv6 eigrp topology 2001:db8:cafe:2::/64**

EIGRP-IPv6 VR(EIGRP\_IPV6) Topology Entry for AS(43)/ID(1.1.1.1) for 2001:DB8:CAFE:2::/64

State is Passive, Query origin flag is 1, 1 Successor(s), FD is 1966080, RIB is 15360

Descriptor Blocks:

FE80::2:1 (Ethernet0/0), from FE80::2:1, Send flag is 0x0

Composite metric is (1966080/1310720), route is Internal

Vector metric:

Minimum bandwidth is 1000000 Kbit

Total delay is 20000000 picoseconds

Reliability is 255/255

Load is 1/255

Minimum MTU is 1500

Hop count is 1

Originating router is 2.2.2.2

FE80::D1:1 (Ethernet0/1.1), from FE80::D1:1, Send flag is 0x0

Composite metric is (2621440/1966080), route is Internal

Vector metric:

Minimum bandwidth is 1000000 Kbit

Total delay is 30000000 picoseconds

Reliability is 255/255

Load is 1/255

Minimum MTU is 1500

Hop count is 2

Originating router is 3.3.3.3

Close configuration window

* 1. **Tune and Optimize EIGRP for IPv6**

In this part of the lab, you will tune and optimize EIGRP for IPv6 through the use of passive interfaces, default router redistribution, summary routes, authentication, load balancing, and route filtering.

* + 1. **Configure specific interfaces as passive.**

Passive interfaces are interfaces that only partially participate in the operation of a routing protocol. The network that a passive interface is connected to is advertised, while the routing protocol does not actually transmit routing protocol-specific traffic on that interface. Use passive interfaces when you have a connected network that you want to advertise, but you do not want protocol neighbors to appear on that interface. Interfaces supporting users should always be configured as passive. There are two ways to configure interfaces as passive. The first is specifically by interface. The other is to make all interfaces default to passive default. Normally a device with many LAN interfaces will use the default option, and then use the **no** form of the command on the specific interfaces that should be sending and receiving EIGRP messages.

* + - 1. On PC1, run Wireshark and set the display capture filter to **eigrp**. You should see a hello message roughly every five seconds. If PC 1 is capable of running EIGRP for IPv6, you might be able to form an adjacency and interact in the routing domain. This is not desirable.
      2. On R1, configure **af-interface E0/1** to be passive.

Open configuration window

R1(config)# **router eigrp EIGRP\_IPV6**

R1(config-router)# **address-family ipv6 unicast autonomous-system 43**

R1(config-router-af)# **af-interface E0/1.2**

R1(config-router-af-interface)# **passive-interface**

R1(config-router-af-interface)# **end**

Close configuration window

* + - 1. On PC1, restart the Wireshark capture with the **eigrp** capture filter. You should no longer see EIGRP Hello messages.
    1. **Configure interfaces from default to passive.**

The second option for configuring passive interfaces is to configure them all as passive and then issue the **no passive-interface** command for certain interfaces. This approach is suitable in a security-focused scenario, or when the device has many LAN interfaces. The commands vary depending on whether you are using Classic or Named EIGRP.

* + - 1. In Classic EIGRP configuration, issue the **passive-interface default** command followed by **no passive-interface [interface designation]** command on the interfaces that should be participating in EIGRP. As an example, configure this on R2, and then make interfaces E0/0 and E0/1 active. Note that you will lose EIGRP adjacencies until the interfaces are active.

Open configuration window

R2(config)# **ipv6 router eigrp 43**

R2(config-rtr)# **passive-interface default**

R2(config-rtr)# **no passive-interface E0/0**

R2(config-rtr)# **no passive-interface E0/1**

R2(config-rtr)# **end**

Close configuration window

* + - 1. In Named EIGRP configuration, you apply the **passive-interface** command to the af-interface default configuration, and then **no passive-interface** command to the af-interface specific interface. On R3, set the af-interface default as passive and then configure E0/0 and S0/1/0 as active. Note that you will lose EIGRP adjacencies until the interfaces are active.

Open configuration window

R3(config)# **router eigrp EIGRP\_IPV6**

R3(config-router)# **address-family ipv6 unicast autonomous-system 43**

R3(config-router-af)# **af-interface default**

R3(config-router-af-interface)# **passive-interface**

R3(config-router-af-interface)# **exit-af-interface**

R3(config-router-af)# **af-interface E0/0**

R3(config-router-af-interface)# **no passive-interface**

R3(config-router-af-interface)# **exit-af-interface**

R3(config-router-af)# **af-interface E0/1**

R3(config-router-af-interface)# **no passive-interface**

R3(config-router-af-interface)# **end**

* + - 1. The output of **show ip protocols | include (passive)** will give you a list of passive interfaces configured for EIGRP.

R3# **show ipv6 protocols | include (passive)**

Loopback5 (passive)

Loopback4 (passive)

Loopback3 (passive)

Loopback2 (passive)

Loopback1 (passive)

Close configuration window

### Propagate a default route.

EIGRP for IPv6 can be configured to propagate a default route to other EIGRP routers in the AS. This lab will explore two methods of propagating a default route, either by redistributing a default static route or by sharing a summary default route.

In this topology, interface Loopback 0 on R2 has been configured to simulate an internet destination. Therefore, we will configure a default route on R2 and then configure EIGRP for IPv6 to redistribute the route.

* + - 1. Configure a static default route on R2 with an exit interface of Loopback0s IPv6 address.

Open configuration window

R2(config)# **ipv6 route ::/0 2001:db8:ff:999::1**

* + - 1. Go into EIGRP configuration add the **redistribute static** command.

R2(config)# **ipv6 router eigrp 43**

R2(config-rtr)# **redistribute static**

R2(config-rtr)# **end**

Close configuration window

* + - 1. At R1, issue the **show ipv6 route eigrp | begin EX ::** command. Notice the default route is present as an EIGRP external route with an AD of 170. Further, notice that individual routes for the 2001:db8:cede::/64 and 2001:db8:cede:1::/64 networks, representing R2 interfaces Lo1 and Lo2, are present in the routing table.

Open configuration window

R1# **show ipv6 route eigrp | begin EX ::**

EX ::/0 [170/2570240]

via FE80::2:1, Ethernet0/0

D 2001:DB8:FF:999::/64 [90/2570240]

via FE80::2:1, Ethernet0/0

D 2001:DB8:ABCD:8::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:9::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:10::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:11::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:12::/64 [90/16000]

via FE80::2:1, Ethernet0/0

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ACAD:3::/64 [90/15360]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:CAFE:2::/64 [90/15360]

via FE80::2:1, Ethernet0/0

D 2001:DB8:CEDE::/64 [90/2570240]

via FE80::2:1, Ethernet0/0

D 2001:DB8:CEDE:1::/64 [90/2570240]

via FE80::2:1, Ethernet0/0

Close configuration window

* + - 1. On R2, remove the **redistribute static** command from EIGRP and remove the static default route.

Open configuration window

* + - 1. On R2, configure the **ipv6 summary-address** command on the Ethernet0/0 and GigabtEthernet0/0/1 interfaces. Specify the eigrp 43 and the route ::/0

R2(config)# **interface Ethernet0/0**

R2(config-if)# **ipv6 summary-address eigrp 43 ::/0**

R2(config-if)# **interface Ethernet0/1**

R2(config-if)# **ipv6 summary-address eigrp 43 ::/0**

Close configuration window

* + - 1. Go to router R1 and use the **show ipv6 route eigrp** command to see the default route that has been injected into the routing table. Notice in the output that the route now appears as an internal EIGRP route with an AD of 90. Also notice that individual routes for the 2001:db8:cede::/64 and 2001:db8:cede:1::/64 networks, representing R2 interfaces Lo1 and Lo2, are no longer present in the routing table. The **ipv6 summary-address ::/0** command replaced all individual routes that R2 was advertising.

**Note**: If you were to add another summary address on R2, similar to what you will do in the next sub-step, that summary would be advertised as well.

Open configuration window

R1# **show ipv6 route eigrp**

<output omitted>

D ::/0 [90/15360]

via FE80::2:1, Ethernet0/0

D 2001:DB8:ABCD:8::/64 [90/16000]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:9::/64 [90/16000]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:10::/64 [90/16000]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:11::/64 [90/16000]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ABCD:12::/64 [90/16000]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ACAD:3::/64 [90/15360]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:CAFE:2::/64 [90/20480]

via FE80::D1:1, Ethernet0/1.1

Close configuration window

* + 1. **Configure an EIGRP for IPv6 Summary Address.**

Router R3 is configured with five loopback interfaces that simulate five IPv6 LANs. Those LAN addresses appear in the other EIGRP routers as five individual routes. In order to limit the impact of these five LANs on routing tables and routing protocol traffic, the routes can be configured with a single route summary address that will enable all five networks to be reached without requiring separate information to be shared for each network.

* + - 1. To optimize EIGRP for IPv6, on R3 summarize the loopback addresses as a single route and advertise the summary route in R3’s EIGRP updates to R1 and R2. Use the same summarization method that is used for IPv4 by finding the bits that all five addresses have in common. The IPv6 loopback addresses could be summarized as 2001:db8:abcd::/61, but common practice is not to split the summary at the nibble level. Therefore, summary masks will normally be 48, 52, 56, and 60 bits. For our exercise, we will specify a 56 bit mask, even though that summary would indicate more networks than R3 is hosting. After configuring the summary route on the interface, notice that the neighbor adjacency between R3 and R2 and R1 is resynchronized (restarted).

Open configuration window

R3(config)# **router eigrp EIGRP\_IPV6**

R3(config-router)# **address-family ipv6 unicast autonomous-system 43**

R3(config-router-af)# **af-interface E0/0**

R3(config-router-af-interface)# **summary-address 2001:db8:abcd::/56**

R3(config-router-af-interface)# **exit**

R3(config-router-af)# **af-interface E0/1**

R3(config-router-af-interface)# **summary-address 2001:db8:abcd::/56**

R3(config-router-af-interface)# **end**

Close configuration window

* + - 1. Examine the routing table of R1 to verify that R1 is receiving only one summary route for the loopback interfaces.

Open configuration window

R1# **show ipv6 route eigrp**

<output omitted>

D ::/0 [90/15360]

via FE80::2:1, Ethernet0/0

D 2001:DB8:ABCD::/56 [90/16000]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:ACAD:3::/64 [90/15360]

via FE80::D1:1, Ethernet0/1.1

D 2001:DB8:CAFE:2::/64 [90/20480]

via FE80::D1:1, Ethernet0/1.1

Close configuration window

* + 1. **Configure EIGRP authentication.**

EIGRP for IPv6 supports authentication on an interface basis. In other words, each interface can be configured to require authentication of the connected peer. This ensures that connected devices that try to form an adjacency are authorized to do so. Classic EIGRP supports key-chain based MD5-hashed keys, while Named EIGRP adds support for SHA256-hashed keys. The two are not compatible.

In this step, you will configure both types of authentication to exercise the range of options available.

* + - 1. On R1, R2, and R3, create a key-chain named EIGRPv6-AUTHEN-KEY with a single key. The key should have the key-string **$3cre7!!**

Open configuration window

R1(config)# **key chain EIGRPv6-AUTHEN-KEY**

R1(config-keychain)# **key 1**

R1(config-keychain-key)# **key-string $3cre7!!**

R1(config-keychain-key)# **end**

Close configuration window

* + - 1. On R2, configure interfaces E0/0 and E0/1 to use the key chain that you just created with MD5. Note that you will lose EIGRP adjacencies until the neighbor interfaces are configured.

Open configuration window

R2(config)# **interface E0/0**

R2(config-if)# **ipv6 authentication key-chain eigrp 43 EIGRPv6-AUTHEN-KEY**

R2(config-if)# **ipv6 authentication mode eigrp 43 md5**

R2(config-if)# **exit**

R2(config)# **interface E0/1**

R2(config-if)# **ipv6 authentication key-chain eigrp 43 EIGRPv6-AUTHEN-KEY**

R2(config-if)# **ipv6 authentication mode eigrp 43 md5**

R2(config-if)# **end**

Close configuration window

* + - 1. Configure interfaces Ethernet0/0 on R1 and R3 to use the key chain with MD5. EIGRP adjacencies with R2 should be restored.

Open configuration window

R1(config)# **router eigrp EIGRP\_IPV6**

R1(config-router)# **address-family ipv6 unicast autonomous-system 43**

R1(config-router-af)# **af-interface E0/0**

R1(config-router-af-interface)# **authentication key-chain EIGRPv6-AUTHEN-KEY**

R1(config-router-af-interface)# **authentication mode md5**

R1(config-router-af-interface)# **end**

* + - 1. Use the **show ip eigrp interface detail** **| section E0/0** command to verify authentication is in place and what type it is.

R1# **show ipv6 eigrp interface detail | section E0/0**

E0/0 1 0/0 0/0 1 0/050 0

Hello-interval is 5, Hold-time is 15

Split-horizon is enabled

Next xmit serial <none>

Packetized sent/expedited: 14/2

Hello's sent/expedited: 186/4

Un/reliable mcasts: 0/11 Un/reliable ucasts: 15/7

Mcast exceptions: 0 CR packets: 0 ACKs suppressed: 0

Retransmissions sent: 3 Out-of-sequence rcvd: 0

Topology-ids on interface - 0

Authentication mode is md5, key-chain is "EIGRP-AUTHEN-KEY"

Topologies advertised on this interface: base

Topologies not advertised on this interface:

* + - 1. On R1, R3 and D2, configure HMAC-SHA-256 based authentication using the same shared secret, **$3cre7!!**, on R1 interface E0/1.1, R3 interface E0/1, and D2 interfaces E1/1 and E1/0. Note that EIGRP adjacency will be lost until both ends of a link are configured.

R1(config)# **router eigrp EIGRP\_IPV6**

R1(config-router)# **address-family ipv6 unicast autonomous-system 43**

R1(config-router-af)# **af-interface E0/1.1**

R1(config-router-af-interface)# **authentication mode hmac-sha-256 $3cre7!!**

R1(config-router-af-interface)# **end**

* + - 1. Use the **show ipv6 eigrp interface detail** command to verify authentication is in place and what type it is.

R1# **show ipv6 eigrp interface detail | section E0/1.1**

E0/1.1 1 0/0 0/0 3 0/050 0

Hello-interval is 5, Hold-time is 15

Split-horizon is enabled

Next xmit serial <none>

Packetized sent/expedited: 27/1

Hello's sent/expedited: 582/3

Un/reliable mcasts: 0/28 Un/reliable ucasts: 35/11

Mcast exceptions: 0 CR packets: 0 ACKs suppressed: 0

Retransmissions sent: 2 Out-of-sequence rcvd: 0

Topology-ids on interface - 0

Authentication mode is HMAC-SHA-256, key-chain is not set

Topologies advertised on this interface: base

Topologies not advertised on this interface:

Close configuration window

* + 1. **Manipulate load balancing with variance.**

By default, load balancing occurs only over equal-cost paths. EIGRP supports up to four equal cost paths by default but can be configured to support as many as 32 with the **maximum-paths** command.

EIGRP has the added capability to load balance over unequal-cost paths. Load balancing is controlled by the **variance** parameter. Its value is a multiplier that is used to determine how to deal with multiple paths to the same destination.

Variance is set to 1 by default, so any paths up to the configured maximum number of paths that have an FD equal to the best current FD are also offered to the routing table. This provides equal cost load balancing.

The variance parameter can also be set to zero, which dictates that no load balancing takes place.

The variance parameter can be adjusted so that paths that have an FD that is less than or equal to variance times current best FD are also considered as successors and installed into the routing table. There is an extremely important differentiation here -- to be a feasible successor, the RD of a path must be less than the current best FD. To be considered for unequal load balancing, the FD of the feasible successor is multiplied by the variance value, and if the product of this calculation is less than the current best FD, the feasible successor is promoted to successor.

There are two caveats; first, only feasible successors are considered and second, with unequal cost load balancing, traffic share is proportional to the best metric in the routing table for the given path.

**Note**: Keep in mind that your routing table may be different than the one created by the examples in this lab. If your results are different, examine them carefully to determine why so that you can thoroughly understand how EIGRP is operating.

* + - 1. Before manipulating variance, R3 needs to see individual routes from R2 instead of a summary. Therefore, remove the summary routes on R2 so that it will again advertise more specific EIGRP routes to R3.

Open configuration window

R2(config-if)# **interface E0/0**

R2(config-if)# **no ipv6 summary-address eigrp 43 ::/0**

R2(config-if)# **exit**

R2(config)# **interface E0/1**

R2(config-if)# **no ipv6 summary-address eigrp 43 ::/0**

R2(config-if)# **end**

Close configuration window

* + - 1. On R3, verify that there are again two equal-cost paths to 2001:db8:acad:2::64. In this example, the IPv6 address must be entered in ALL CAPS.

Open configuration window

R3# **show ipv6 route eigrp | section 2001:DB8:ACAD:2::/64**

D 2001:DB8:ACAD:2::/64 [90/20480]

via FE80::D1:2, Ethernet0/1

via FE80::2:2, Ethernet0/0

Close configuration window

* + - 1. To change this and allow for the demonstration of variance, change the interface bandwidth for the R2 interfaces E0/0 and E0/1 to 800000.

Open configuration window

R2(config)# **interface E0/0**

R2(config-if)# **bandwidth 800000**

R2(config-if)# **exit**

R2(config)# **interface E0/1**

R2(config-if)# **bandwidth 800000**

R2(config-if)# **end**

Close configuration window

* + - 1. When you examine the routing table on R3, you see that there is no load balancing occurring. All destinations have a single path.

Open configuration window

R3# **show ipv6 route eigrp | section 2001:DB8:ACAD:2::/64**

D 2001:DB8:ACAD:2::/64 [90/20480]

via FE80::D1:2, Ethernet0/1

* + - 1. However, we know there are multiple paths in the network. The first consideration for manipulating variance is that it only works with feasible successors. Examining the topology table on R3 shows that there is a feasible successor for the 2001:db8:acad:2::/64 network. The route via fe80::2:2 out the E0/0 interface has an RD less than the FD for the current successor.

R3# **show ipv6 eigrp topology | section 2001:DB8:ACAD:2::/64**

P 2001:DB8:ACAD:2::/64, 1 successors, FD is 2621440

via FE80::D1:2 (2621440/1966080), Ethernet0/1

via FE80::2:2 (2785280/2129920), Ethernet0/0

* + - 1. To use the other route for unequal cost load balancing, we can set the variance parameter to 2. This will mean that any path with an RD less than or equal to 5242880 will qualify as a successor (2 x 2621440 = 5242880).

R3(config)# **router eigrp EIGRP\_IPV6**

R3(config-router)# **address-family ipv6 unicast autonomous-system 43**

R3(config-router-af)# **topology base**

R3(config-router-af-topology)# **variance 2**

R3(config-router-af-topology)# **exit**

R3(config-router-af)# **exit**

R3(config-router)# **exit**

R3(config)# **end**

* + - 1. The output of the **show ipv6 route eigrp** command now displays two paths available to the 2001:db8:acad:2::/64 network. Notice that the routes have different metrics, but are listed and used just the same. Also, notice adding **variance 2** adds a second path to the 2001:db8:cafe:1::/64 network.

R3# **show ipv6 route eigrp**

<output omitted>

D 2001:DB8:FF:999::/64 [90/2570240]

via FE80::2:2, Ethernet0/0

D 2001:DB8:ABCD::/56 [5/1280]

via Null0, directly connected

D 2001:DB8:ACAD:2::/64 [90/20480]

via FE80::D1:2, Ethernet0/1

via FE80::2:2, Ethernet0/0

D 2001:DB8:ACAD:3::/64 [90/15360]

via FE80::D1:2, Ethernet0/1

D 2001:DB8:CAFE:1::/64 [90/16640]

via FE80::2:2, Ethernet0/0

via FE80::D1:2, Ethernet0/1

D 2001:DB8:CEDE::/64 [90/2570240]

via FE80::2:2, Ethernet0/0

D 2001:DB8:CEDE:1::/64 [90/2570240]

via FE80::2:2, Ethernet0/0

### Filter EIGRP routes using a prefix list.

In this step, you will configure a filter at R2 to block propagation of the network 2001:db8:cafe:1::/64 to R3.

* + - 1. On R3, issue the command **show ipv6 route 2001:db8:cafe:1::/64** command. The output should list two successors, one via fe80::2:2 and one via fe90::d2:2. We want to filter route via fe80::2:1.

R3# **show ipv6 route 2001:db8:cafe:1::/64**

Routing entry for 2001:DB8:CAFE:1::/64

Known via "eigrp 43", distance 90, metric 16640, type internal

Route count is 2/2, share count 0

Routing paths:

FE80::2:2, Ethernet0/0

From FE80::2:2

Last updated 00:05:00 ago

FE80::D1:2, Ethernet0/1

From FE80::D1:2

Last updated 00:04:35 ago

Close configuration window

* + - 1. On R2, create an IPv6 prefix list that matches the 2001:db8:cafe:1::/64 network.

Open configuration window

R2(config)# **ipv6 prefix-list DROP-CAFE-1 seq 10 deny 2001:db8:cafe:1::/64**

R2(config)# **ipv6 prefix-list DROP-CAFE-1 seq 20 permit ::/0**

R2(config)# **end**

* + - 1. On R2, apply the prefix list as a distribute list for updates exiting the E0/1 interface towards R3.

R2(config)# **ipv6 router eigrp 43**

R2(config-rtr)# **distribute-list prefix-list DROP-CAFE-1 out E0/1**

R2(config-rtr)# **exit**

R2(config)# **end**

Close configuration window

* + - 1. On R3, issue the **show ipv6 route 2001:db8:cafe:1::/64** command. The output should now list one successor fe80::d1:2. Verify that R3 no longer has a successor route via fe80::2:2 to the 2001:db8:cafe:1::/64 network.

Open configuration window

R3# **show ipv6 route 2001:db8:cafe:1::/64**

Routing entry for 2001:DB8:CAFE:1::/64

Known via "eigrp 43", distance 90, metric 20480, type internal

Route count is 1/1, share count 0

Routing paths:

FE80::D1:2, Ethernet0/1

From FE80::D1:2

Last updated 00:15:29 ago

Close configuration window

# Router Interface Summary Table

| Router Model | Ethernet Interface #1 | Ethernet Interface #2 | Serial Interface #1 | Serial Interface #2 |
| --- | --- | --- | --- | --- |
| 1800 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 1900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2801 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 2811 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 4221 | Gigabit Ethernet 0/0/0 (E0/0) | Gigabit Ethernet 0/0/1 (E0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 4300 | Gigabit Ethernet 0/0/0 (E0/0) | Gigabit Ethernet 0/0/1 (E0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |

**Note**: To find out how the router is configured, look at the interfaces to identify the type of router and how many interfaces the router has. There is no way to effectively list all the combinations of configurations for each router class. This table includes identifiers for the possible combinations of Ethernet and Serial interfaces in the device. The table does not include any other type of interface, even though a specific router may contain one. An example of this might be an ISDN BRI interface. The string in parenthesis is the legal abbreviation that can be used in Cisco IOS commands to represent the interface.

End of document