
Lab - Configure Secure DMVPN Tunnels

# Topology



# Addressing Table

| **Device** | **Interface** | **IPv4 Address** |
| --- | --- | --- |
| R1 | G0/0/1 | 192.0.2.1/24 |
| R1 | Tunnel 1 | 100.100.100.1/29 |
| R2 | G0/0/1 | 198.51.100.2/24 |
| R2 | Loopback 0 | 192.168.1.1/24 |
| R2 | Loopback 1 | 172.16.1.1/24 |
| R2 | Tunnel 1 | 100.100.100.2/29 |
| R3 | G0/0/1 | 203.0.113.2/24 |
| R3 | Loopback 0 | 192.168.3.1/24 |
| R3 | Loopback 1 | 172.16.3.1/24 |
| R3 | Tunnel 1 | 100.100.100.3/29 |

# Objectives

Part 1: Build the Network and Verify DMVPN Phase 3 Operation

Part 2: Secure DMVPN Phase 3 Tunnels

# Background / Scenario

In previous labs, you have configured DMVPN Phase 1 and Phase 3 networks, including configuration of DMVPN Phase 3 with IPv6. However, in those labs, IPsec was not used to encrypt and protect data travelling on the tunnels. IPsec functionality is essential to DMVPN implementation. In this lab, you will work with the DMVPN Phase 3 implementation from the Implement a DMVPN Phase 3 Spoke-to-Spoke Topology lab. You will start with a working configuration and then apply IPsec to the spoke-to-hub and spoke-to-spoke tunnels. Finally, you will verify the operation of the secured tunnels.

**Note**: The routers used with CCNA hands-on labs are Cisco 4221 with Cisco IOS XE Release 16.9.4 (universalk9 image). The switch used is a Cisco Catalyst 3650 with Cisco IOS XE Release 16.9.4 (universalk9 image). Other routers, Layer 3 switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of the lab for the correct interface identifiers.

# Required Resources

* 3 Routers (Cisco 4221 with Cisco IOS XE Release 16.9.4 universal image or comparable)
* 1 Switch (Cisco 3560 with Cisco IOS XE Release 16.9.4 universal image or comparable)
* 1 PC (Choice of operating system with a terminal emulation program installed)
* Console cables to configure the Cisco IOS devices via the console ports
* Ethernet cables as shown in the topology

# Instructions

## Build the Network and Verify DMVPN Phase 3 Operation

In Part 1, you will set up the network topology and configure basic settings if the network is not already configured. This lab uses the same topology and final configurations from the **Implement a DMVPN Phase 3 Spoke-to-Spoke Topology** lab.

### Cable the network as shown in the topology.

Connect the devices as shown in the topology diagram.

### Configure initial settings for each router and the Layer 3 switch.

Console into each device, enter global configuration mode, and apply the initial settings for the lab if the devices are not already configured.

### Verify connectivity in the network.

* + - 1. From R1, **ping** the loopback interfaces of R2 and R3. All pings should be successful. This verifies that full connectivity exists in the underlay, or transport, network.

Open configuration window

R1# **ping 192.168.2.1**

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 192.168.3.1, timeout is 2 seconds:

!!!!!

Success rate is 100 percent (5/5), round-trip min/avg/max = 1/1/1 ms

R1# **ping 192.168.3.1**

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 192.168.3.1, timeout is 2 seconds:

!!!!!

Success rate is 100 percent (5/5), round-trip min/avg/max = 1/1/1 ms

Close configuration window

### Verify DMVPN Phase 3 operation.

* + - 1. Return to R2. Initiate a **traceroute** to the simulated LAN interface on R3. The path will pass through R1 as it does in a DMVPN Phase 1 network.

**Note**: The first trace may fail if the DMVPN switch CAM table is empty.

Open configuration window

R2# **traceroute 172.16.3.1**

Type escape sequence to abort.

Tracing the route to 172.16.3.1

VRF info: (vrf in name/id, vrf out name/id)

1 100.100.100.1 1 msec 1 msec 1 msec

2 100.100.100.3 1 msec \* 2 msec

* + - 1. Issue the **traceroute** command again. You will now see that R1 has enabled direct spoke-to-spoke communication between R2 and R3. This tunnel will expire and close dynamically. The tunnel reopens after data for the spoke router is sent again.

R2# **traceroute 172.16.3.1**

Type escape sequence to abort.

Tracing the route to 172.16.3.1

VRF info: (vrf in name/id, vrf out name/id)

1 100.100.100.3 1 msec \* 1 msec

Close configuration window

## Secure DMVPN Phase 3 Tunnels

Now that the tunnels have been configured and DMVPN connectivity has been verified, the tunnels can be secured with IPsec.

### Create the IKE policy.

Create an IKE policy that defines the hash algorithm, encryption type, key exchange method, Diffie-Hellman group, and the authentication method.

Open configuration window

R1(config)# **crypto isakmp policy 99**

R1(config-isakmp)# **hash sha384**

R1(config-isakmp)# **encryption aes 256**

R1(config-isakmp)# **group 14**

R1(config-isakmp)# **authentication pre-share**

R1(config-isakmp)# **exit**

### Configure the ISAKMP key.

Configure the pre-shared key and peer address. Use 0.0.0.0 to match multiple peer addresses. Use a key of **DMVPN@key#**.

R1(config)# **crypto isakmp key DMVPN@key# address 0.0.0.0**

### Create and configure the IPsec transform set.

Configure the IPsec transform set. Use **DMVPN\_TRANS** as the transform set name. Specify **esp-aes** with a 256-bit key as the encryption transform and **esp-sha384-hmac** as the authentication transform. Configure the transform set to use IPsec **transport** mode for the tunnels.

R1(config)# **crypto ipsec transform-set DMVPN\_TRANS esp-aes 256 esp-sha384-hmac**

R1(cfg-crypto-trans)# **mode transport**

R1(cfg-crypto-trans)# **exit**

### Create the IPsec profile.

Create an IPsec profile with the name **DMVPN\_PROFILE**. Associate the **DMVPN\_TRANS** transform set with the profile.

R1(config)# **crypto ipsec profile DMVPN\_PROFILE**

R1(ipsec-profile)# **set transform-set DMVPN\_TRANS**

R1(ipsec-profile)# **exit**

### Apply the IPsec profile to the tunnel interface.

Finally, apply the IPsec profile to the tunnel interface. After you apply the profile, you will see the that IPsec is now active and you will lose adjacency with R2 and R3 until their respective ends of the tunnel are configured.

R1(config)# **interface tunnel 1**

R1(config-if)# **tunnel protection ipsec profile DMVPN\_PROFILE**

R1(config-if)# **exit**

\*Mar 30 07:39:32.398: %CRYPTO-6-ISAKMP\_ON\_OFF: ISAKMP is ON

R1(config)#

\*Mar 30 07:39:32.963: %IOSXE-3-PLATFORM: R0/0: cpp\_cp: QFP:0.0 Thread:001 TS:00000000594132950499 %IPSEC-3-RECVD\_PKT\_NOT\_IPSEC: Rec'd packet not an IPSEC packet, dest\_addr= 192.0.2.1, src\_addr= 192.168.2.1, prot= 47

\*Mar 30 07:39:43.664: %DUAL-5-NBRCHANGE: EIGRP-IPv4 68: Neighbor 100.100.100.2 (Tunnel1) is down: holding time expired

\*Mar 30 07:39:44.235: %DUAL-5-NBRCHANGE: EIGRP-IPv4 68: Neighbor 100.100.100.3 (Tunnel1) is down: holding time expired

R1(config)#

Close configuration window

### Configure R2 and R3 with IPsec.

Repeat this configuration on the R2 and R3 routers.

### Verify DMVPN Phase 3 operation.

* + - 1. As was done previously, test the operation of the spoke-to-spoke DMVPN. Return to R2. Initiate a **traceroute** to the simulated LAN interface on R3. The path will pass through R1 as it does in a DMVPN Phase 1 network.

Open configuration window

R2# **traceroute 172.16.3.1**

Type escape sequence to abort.

Tracing the route to 172.16.3.1

VRF info: (vrf in name/id, vrf out name/id)

1 100.100.100.1 1 msec 1 msec 1 msec

2 100.100.100.3 1 msec \* 2 msec

* + - 1. Issue the **traceroute** command again. You will now see that R1 has enabled direct spoke-to-spoke communication between R2 and R3. This tunnel will expire and close dynamically. The tunnel reopens after data for the spoke router is sent again.

R2# **traceroute 172.16.3.1**

Type escape sequence to abort.

Tracing the route to 172.16.3.1

VRF info: (vrf in name/id, vrf out name/id)

1 100.100.100.3 1 msec \* 1 msec

### Verify IPsec configuration.

**Note**: Shut down a tunnel interface to clear its IPsec socket if you wish to explore the outputs before and after spoke-to-spoke tunnel establishment.

* + - 1. To show information about the IPsec profiles that are configured on a device, issue the **show crypto ipsec profile** command. Note that the profile that was previously configured is shown along with a default profile.

R2# **show crypto ipsec profile**

IPSEC profile DMVPN\_PROFILE

Security association lifetime: 4608000 kilobytes/3600 seconds

Responder-Only (Y/N): N

PFS (Y/N): N

Mixed-mode : Disabled

Transform sets={

DMVPN\_TRANS: { esp-256-aes esp-sha384-hmac } ,

}

IPSEC profile default

Security association lifetime: 4608000 kilobytes/3600 seconds

Responder-Only (Y/N): N

PFS (Y/N): N

Mixed-mode : Disabled

Transform sets={

default: { esp-aes esp-sha-hmac } ,

}

Close configuration window

* + - 1. It is very important to verify that tunnel traffic will be encrypted. On R1, issue the **show dmvpn detail** command. As the hub router, R1 should see the spoke peers. The first part of the output shows the tunnel interface status and the peer table. Both peers should be shown with their transport and overlay interface addresses, as you have seen previously.

The Crypto Session Details portion of the output should contain information about the status of the encrypted tunnels. Both of the spoke routers should appear in this output also. Note that the transform set that you configured is also displayed in the Crypto Session output.

Open configuration window

R1# **show dmvpn detail**

<output omitted>

Interface Tunnel1 is up/up, Addr. is 100.100.100.1, VRF ""

Tunnel Src./Dest. addr: 192.0.2.1/Multipoint, Tunnel VRF ""

Protocol/Transport: "multi-GRE/IP", Protect "DMVPN\_PROFILE"

Interface State Control: Disabled

nhrp event-publisher : Disabled

Type:Hub, Total NBMA Peers (v4/v6): 2

# Ent Peer NBMA Addr Peer Tunnel Add State UpDn Tm Attrb Target Network

----- --------------- --------------- ----- -------- ----- -----------------

1 192.168.2.1 100.100.100.2 UP 00:04:25 D 100.100.100.2/32

1 192.168.3.1 100.100.100.3 UP 00:04:59 D 100.100.100.3/32

Crypto Session Details:

--------------------------------------------------------------------------------

Interface: Tunnel1

Session: [0x7F6E17B867D0]

Session ID: 0

IKEv1 SA: local 192.0.2.1/500 remote 192.168.2.1/500 Active

Capabilities:(none) connid:1001 lifetime:23:59:19

Session ID: 0

IKEv1 SA: local 192.0.2.1/500 remote 192.168.2.1/500 Active

Capabilities:(none) connid:1002 lifetime:23:59:28

Crypto Session Status: UP-ACTIVE

fvrf: (none), Phase1\_id: 192.168.2.1

IPSEC FLOW: permit 47 host 192.0.2.1 host 192.168.2.1

Active SAs: 4, origin: crypto map

Inbound: #pkts dec'ed 17 drop 0 life (KB/Sec) 4607998/3568

Outbound: #pkts enc'ed 16 drop 0 life (KB/Sec) 4607999/3568

Outbound SPI : 0xD2E76488, transform : esp-256-aes esp-sha384-hmac

Socket State: Open

Interface: Tunnel1

Session: [0x7F6E17B86950]

Session ID: 0

IKEv1 SA: local 192.0.2.1/500 remote 192.168.3.1/500 Active

Capabilities:(none) connid:1004 lifetime:23:59:48

Session ID: 0

IKEv1 SA: local 192.0.2.1/500 remote 192.168.3.1/500 Active

Capabilities:(none) connid:1003 lifetime:23:59:40

Crypto Session Status: UP-ACTIVE

fvrf: (none), Phase1\_id: 192.168.3.1

IPSEC FLOW: permit 47 host 192.0.2.1 host 192.168.3.1

Active SAs: 6, origin: crypto map

Inbound: #pkts dec'ed 11 drop 0 life (KB/Sec) 4607999/3588

Outbound: #pkts enc'ed 10 drop 0 life (KB/Sec) 4607999/3588

Outbound SPI : 0xCB3D3313, transform : esp-256-aes esp-sha384-hmac

Socket State: Open

Pending DMVPN Sessions:

Close configuration window

* + - 1. Issue the **show crypto ipsec sa** command on R2 to display the security associations (sa) that have been made by R2. This output is for the spoke-to-hub tunnel between R1 and R2 prior to the establishment of the spoke-to-spoke tunnel. This command provides additional details regarding the IPsec status of the tunnel, encrypted and decrypted packet statistics, and other details regarding characteristics of the encrypted tunnel.

Open configuration window

R2# **show crypto ipsec sa**

interface: Tunnel1

Crypto map tag: Tunnel1-head-0, local addr 192.168.2.1

protected vrf: (none)

local ident (addr/mask/prot/port): (192.168.2.1/255.255.255.255/47/0)

remote ident (addr/mask/prot/port): (192.0.2.1/255.255.255.255/47/0)

current\_peer 192.0.2.1 port 500

PERMIT, flags={origin\_is\_acl,}

#pkts encaps: 125, #pkts encrypt: 125, #pkts digest: 125

#pkts decaps: 126, #pkts decrypt: 126, #pkts verify: 126

#pkts compressed: 0, #pkts decompressed: 0

#pkts not compressed: 0, #pkts compr. failed: 0

#pkts not decompressed: 0, #pkts decompress failed: 0

#send errors 0, #recv errors 0

local crypto endpt.: 192.168.2.1, remote crypto endpt.: 192.0.2.1

plaintext mtu 1458, path mtu 1514, ip mtu 1514, ip mtu idb Loopback0

current outbound spi: 0x97C1D18A(2546061706)

PFS (Y/N): N, DH group: none

inbound esp sas:

spi: 0xD2E76488(3538379912)

transform: esp-256-aes esp-sha384-hmac ,

in use settings ={Transport, }

conn id: 2003, flow\_id: ESG:3, sibling\_flags FFFFFFFF80000008, crypto map: Tunnel1-head-0

sa timing: remaining key lifetime (k/sec): (4607984/3047)

IV size: 16 bytes

replay detection support: Y

Status: ACTIVE(ACTIVE)

inbound ah sas:

inbound pcp sas:

outbound esp sas:

spi: 0x97C1D18A(2546061706)

transform: esp-256-aes esp-sha384-hmac ,

in use settings ={Transport, }

conn id: 2004, flow\_id: ESG:4, sibling\_flags FFFFFFFF80000008, crypto map: Tunnel1-head-0

sa timing: remaining key lifetime (k/sec): (4607990/3047)

IV size: 16 bytes

replay detection support: Y

Status: ACTIVE(ACTIVE)

outbound ah sas:

outbound pcp sas:

The output below is for the same command after the spoke-to-spoke tunnel is open. Entries exist for both the tunnel to R1 and the spoke-to-spoke tunnel between R2 and R3.

R2# **show crypto ipsec sa**

interface: Tunnel1

Crypto map tag: Tunnel1-head-0, local addr 192.168.2.1

protected vrf: (none)

local ident (addr/mask/prot/port): (192.168.2.1/255.255.255.255/47/0)

remote ident (addr/mask/prot/port): (192.168.3.1/255.255.255.255/47/0)

current\_peer 192.168.3.1 port 500

PERMIT, flags={origin\_is\_acl,}

#pkts encaps: 0, #pkts encrypt: 0, #pkts digest: 0

#pkts decaps: 0, #pkts decrypt: 0, #pkts verify: 0

#pkts compressed: 0, #pkts decompressed: 0

#pkts not compressed: 0, #pkts compr. failed: 0

#pkts not decompressed: 0, #pkts decompress failed: 0

#send errors 0, #recv errors 0

local crypto endpt.: 192.168.2.1, remote crypto endpt.: 192.168.3.1

plaintext mtu 1458, path mtu 1514, ip mtu 1514, ip mtu idb Loopback0

current outbound spi: 0x658E8CF5(1703841013)

PFS (Y/N): N, DH group: none

inbound esp sas:

spi: 0xFA8FC9F2(4203727346)

transform: esp-256-aes esp-sha384-hmac ,

in use settings ={Transport, }

conn id: 2005, flow\_id: ESG:5, sibling\_flags FFFFFFFF80000008, crypto map: Tunnel1-head-0

sa timing: remaining key lifetime (k/sec): (4608000/3316)

IV size: 16 bytes

replay detection support: Y

Status: ACTIVE(ACTIVE)

spi: 0x59C41A42(1506024002)

transform: esp-256-aes esp-sha384-hmac ,

in use settings ={Transport, }

conn id: 2007, flow\_id: ESG:7, sibling\_flags FFFFFFFF80004008, crypto map: Tunnel1-head-0

sa timing: remaining key lifetime (k/sec): (4608000/3326)

IV size: 16 bytes

replay detection support: Y

Status: ACTIVE(ACTIVE)

inbound ah sas:

inbound pcp sas:

outbound esp sas:

spi: 0x60CC6F77(1624010615)

transform: esp-256-aes esp-sha384-hmac ,

in use settings ={Transport, }

conn id: 2006, flow\_id: ESG:6, sibling\_flags FFFFFFFF80000008, crypto map: Tunnel1-head-0

sa timing: remaining key lifetime (k/sec): (4608000/3316)

IV size: 16 bytes

replay detection support: Y

Status: ACTIVE(ACTIVE)

spi: 0x658E8CF5(1703841013)

transform: esp-256-aes esp-sha384-hmac ,

in use settings ={Transport, }

conn id: 2008, flow\_id: ESG:8, sibling\_flags FFFFFFFF80004008, crypto map: Tunnel1-head-0

sa timing: remaining key lifetime (k/sec): (4608000/3326)

IV size: 16 bytes

replay detection support: Y

Status: ACTIVE(ACTIVE)

outbound ah sas:

outbound pcp sas:

protected vrf: (none)

local ident (addr/mask/prot/port): (192.168.2.1/255.255.255.255/47/0)

remote ident (addr/mask/prot/port): (192.0.2.1/255.255.255.255/47/0)

current\_peer 192.0.2.1 port 500

PERMIT, flags={origin\_is\_acl,}

#pkts encaps: 67, #pkts encrypt: 67, #pkts digest: 67

#pkts decaps: 67, #pkts decrypt: 67, #pkts verify: 67

#pkts compressed: 0, #pkts decompressed: 0

#pkts not compressed: 0, #pkts compr. failed: 0

#pkts not decompressed: 0, #pkts decompress failed: 0

#send errors 0, #recv errors 0

local crypto endpt.: 192.168.2.1, remote crypto endpt.: 192.0.2.1

plaintext mtu 1458, path mtu 1514, ip mtu 1514, ip mtu idb Loopback0

current outbound spi: 0x97C1D18A(2546061706)

PFS (Y/N): N, DH group: none

inbound esp sas:

spi: 0xD2E76488(3538379912)

transform: esp-256-aes esp-sha384-hmac ,

in use settings ={Transport, }

conn id: 2003, flow\_id: ESG:3, sibling\_flags FFFFFFFF80000008, crypto map: Tunnel1-head-0

sa timing: remaining key lifetime (k/sec): (4607991/3305)

IV size: 16 bytes

replay detection support: Y

Status: ACTIVE(ACTIVE)

inbound ah sas:

inbound pcp sas:

outbound esp sas:

spi: 0x97C1D18A(2546061706)

transform: esp-256-aes esp-sha384-hmac ,

in use settings ={Transport, }

conn id: 2004, flow\_id: ESG:4, sibling\_flags FFFFFFFF80000008, crypto map: Tunnel1-head-0

sa timing: remaining key lifetime (k/sec): (4607995/3305)

IV size: 16 bytes

replay detection support: Y

Status: ACTIVE(ACTIVE)

outbound ah sas:

outbound pcp sas:

* + - 1. On R2 issue the **show crypto isakmp sa** commandto view theInternet Security Association Management Protocol (ISAKMP) SAs between the peers. Before the formation of the spoke-to-spoke tunnel, SAs have been made between R2 and R3, but no further negotiations have occurred, as indicated by the MM\_NO\_STATE state of the two SAs between the routers.

R2# **show crypto isakmp sa**

IPv4 Crypto ISAKMP SA

dst src state conn-id status

192.0.2.1 192.168.2.1 QM\_IDLE 1001 ACTIVE

192.168.2.1 192.0.2.1 QM\_IDLE 1002 ACTIVE

192.168.3.1 192.168.2.1 MM\_NO\_STATE 1004 ACTIVE (deleted)

192.168.2.1 192.168.3.1 MM\_NO\_STATE 1003 ACTIVE (deleted)

IPv6 Crypto ISAKMP SA

After traffic has established the spoke-to-spoke tunnel, the SAs all show the QM\_IDLE state. The SAs have been fully negotiated and are available for further ISAKMP quick mode exchanges.

**Note**: ISAKMP modes are outside the scope of this course.

R2# **show crypto isakmp sa**

IPv4 Crypto ISAKMP SA

dst src state conn-id status

192.0.2.1 192.168.2.1 QM\_IDLE 1001 ACTIVE

192.168.2.1 192.0.2.1 QM\_IDLE 1002 ACTIVE

192.168.3.1 192.168.2.1 QM\_IDLE 1004 ACTIVE

192.168.2.1 192.168.3.1 QM\_IDLE 1003 ACTIVE

IPv6 Crypto ISAKMP SA

* + - 1. You have successfully configured and verified IPsec on DMVPN Phase 3 tunnels.

Close configuration window

# Router Interface Summary Table

| Router Model | Ethernet Interface #1 | Ethernet Interface #2 | Serial Interface #1 | Serial Interface #2 |
| --- | --- | --- | --- | --- |
| 1800 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 1900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2801 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 2811 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 4221 | Gigabit Ethernet 0/0/0 (G0/0/0) | Gigabit Ethernet 0/0/1 (G0/0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 4300 | Gigabit Ethernet 0/0/0 (G0/0/0) | Gigabit Ethernet 0/0/1 (G0/0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |

**Note**: To find out how the router is configured, look at the interfaces to identify the type of router and how many interfaces the router has. There is no way to effectively list all the combinations of configurations for each router class. This table includes identifiers for the possible combinations of Ethernet and Serial interfaces in the device. The table does not include any other type of interface, even though a specific router may contain one. An example of this might be an ISDN BRI interface. The string in parenthesis is the legal abbreviation that can be used in Cisco IOS commands to represent the interface.

End of document